VGA output

In 16 bit INT VGA color

Kernel

File system

External process handler, command intepreter, and executer

Timing handler, multitasking handler and process counter

Kernel interac. Lay.

Temp

Var storage

tcpip

User Prompt CCL (c command line)

Translator and Interpreter

DB9 serial

Keyboard

MINIX / SFS / FAT12 support

Transfer variables over serial (serial interpreter raw)

Get interaction from serial port / send out serial raw

Get multicolored output, 16bit vga colors.

Successful user interaction with computer (kb)

Successful saving of user input in variable.

Get the first version of kernel to boot and output.